**[Part ID: 230400 - MAC Bucket with Rubber Auger](https://www.danuser.com/product/918)**

A diagram of a machine

AI-generated content may be incorrect.

* **Capacity**

1/2 yard (13.5 cubic ft.); up to 3/4 yard (20 cubic ft.) with optional hopper extension

* **Concrete Mix Capacity (80-lb bags)**

Approx. 18 (1/2 yd)  
Approx. 25 (3/4 yd)

* **Dispense Rate**

28 seconds @ 24 GPM

* **Hydraulic Requirements**

Up to 24 GPM  
Up to 3,500 PSI

* **Mounting Options**

Skid-Steer Quick Attach

* **Height, Grate Lowered (A) (inches)**

33.5"

* **Height, Grate Open (B) (inches)**

47"

* **Overall Width (C) (inches)**

26"

* **Overall Length (D) (inches)**

77.4"

* **Overall Hopper Length (E) (inches)**

71.3"

* **Weight**

615 lb.

* **Auger Diameter without Rubber (inches)**

4"

* **Auger Diameter with Rubber (inches)**

6.5"

* **Center Column Diameter (inches)**

1.32" O.D.  
.18" wall

* **Auger Length (inches)**

60"

* **Flighting Spacing (inches)**

4"